IHOP_2002_S5_TRM
Percent Volumetric Soil Moisture Content as measured with the Trime TDR Probe.

Site:	5

Date:	Given as MMDDYY

Time	Given as HHmmss	
			Note:	The time is in GMT (Local Time (CDT) + 5 hours
				Second of measurement not recorded; 00 added to time to maintain format

				Time and Data indicate the beginning of the measurement.

Location	1-10	Single E to W transect (1) is nearest flux tower
	11	In view of IR thermometer on flux tower - no Trime measurements made at this location
	12	Soil Probes at the foot of the Radiometer Stand
	13	Soil Profiler12
	14-15	No additional soil profilers at this site
	16	Location of Gravimetric Soil Core


Error Codes	999998	Measurement not applicable
		999999	Data Missing


Trime Collected On: 05/22/02	05/28/02	06/05/02	06/12/02

Probe inserted into the soil at a 45 degree angle. 
Samples were recorded after the reading had stablized, typically 30 to 60 seconds.

JGA 